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Scope
This Section specifies health and safety administrative requirements for contractors performing work for the Region of Durham.
References
Occupational Health and Safety Act, R.S.O. 1990, c. O.1 (OHSA).
Ontario Regulation 213/91 (Construction Projects) made under the Occupational Health and Safety Act.
Ontario Regulation 632/05 (Confined Spaces) made under the Occupational Health and Safety Act.
General requirements
Provide a copy of Contractor’s current health and safety policies and program. Implement these policies prior to the commencement of construction.
Upon request, provide copies of all Subcontractors’ health and safety policies and programs prior to such Subcontractor commencing work on the site.
Comply with all federal and provincial health and safety acts, regulations and lower tier municipality by-laws and with all applicable industry safety standards.
Provide all personal protective equipment for Contractor’s own workers where prescribed.
Provide to the Consultant a list of designated substances that will be brought to the site prior to commencing work. Safety Data Sheets (SDS) and the hazardous material inventory for each substance listed must be kept on the Project.
Maintain current SDS on site at a location accessible to all workers, the Consultant and the Owner.
In event of conflict between any provisions of above authorities, the most stringent provision governs.
List of designated substances at the site
In accordance with the requirements of Section 30 of the OHSA, the Bidder is hereby advised that the designated substances as listed hereunder are or may be present on the site and within the limits of this Contract:
	Designated substance
	Identified on this site?
Indicate: Yes / No / Not identified
	Location on site

	Acrylonitrile
	
	

	Arsenic
	
	

	Asbestos
	
	

	Benzene
	
	

	Coke Oven Emissions
	
	

	Ethylene Oxide
	
	

	Isocyanate
	
	

	Lead
	
	

	Mercury
	
	

	Silica
	
	

	Vinyl Chloride
	
	


The Contractor shall comply with the governing Ministry of Labour regulations respecting protection of workers, removal, handling and disposition of any designated substances encountered in carrying out the Work proposed on this contract.
Prior to commencement of this work, provide written notification to the Ministry of the Environment, Conservation and Parks (MECP) at their district office of the location(s) proposed for disposal of designated substances. Provide a copy of the notification to the Consultant a minimum of two weeks in advance of such work starting.
In the event that the MECP has concerns with any proposed disposal location, further notification shall be provided until the MECP’s concerns have been addressed.
Should a designated substance not herein identified be encountered in the Work, then management of such substance shall be treated as Extra Work.
Designated Substances Reports have been included in Appendix D2 – Material Disclosures of the tender documents for bidders’ review and consideration.
Health and safety warnings
The Consultant and the Owner shall have the right to document all Contractors for all health and safety warnings and/or to stop any Contractor’s work if the Contractor fails to comply with any requirements under this section.
Similarly, the Consultant and the Owner shall have the right to issue warnings and/or to stop work for any Contractor violations of the contract and/or if the Contractor creates a health or safety hazard.
Written warnings and/or stop work orders shall be given to the Contractor using the Owner’s Contractor Health and Safety Warning / Stop Work Order Form.
If the Contractor fails to adequately respond to the Consultant’s or the Owner’s order to correct a hazard in accordance with CCDC 2 2020 GC 9.4 as amended by the Supplementary Conditions, the Owner reserves the right to have the hazard corrected by a third party at the Contractor’s expense. The Consultant’s or the Owner’s decision, as the case may be, as to the urgency for such correction shall be final.
Notice of project
Notify all regulatory bodies required for construction activities, (e.g., Notice of Project, employer notification, etc.). Notifications shall include, but not be limited to, the notification requirements laid out in OHSA Section 51 through Section 53.1 and the requirements of Ontario Regulation 213/91 (Construction Projects) Sections 5, 6 and 7. For the purpose of this contract the Contractor shall be the “Constructor”.
Confined space
Persons intended to work in confined spaces as defined by Ontario Regulation 632/05 (Confined Spaces) must have formal training in performing work in confined spaces.
Provide proof of valid certificates of such training for all workers prior to entry of such workers into confined spaces.
Provide all necessary safety equipment for entry into confined spaces.
Where workers are required to enter a confined space, ensure that workers of the Contractor and all Subcontractors follow the requirements of the above legislation, including but not limited to:
Having a method for recognizing each confined space to which the program applies.
Having a method for assessing the hazards to which workers may be exposed.
Having a method for the development of confined space entry plans (which include on-site rescue procedures).
Having a method for training workers.
Having an entry permit system.
Supply the necessary tools and equipment to perform the confined space entry. These items include, but are not limited to, required documentation, gas detectors, breathing equipment, fall protection and rescue equipment.
Working at heights
At a minimum, systems and devices for fall prevention and/or fall arrest shall be used and/or worn for any Work activity where a worker may fall a vertical distance, as outlined in the most stringent requirement listed in all applicable Acts or other applicable regulations.
1.1 Site Conditions
Work on this site may involve contact with:
1. Aluminum sulphate
Chlorine gas
Diesel fuel
Hydrofluosilicic Acid
Sodium bisulphite
Other substances listed in the Plant’s Designated Substance Survey 
High noise areas
.1 The Contractor shall be responsible for supplying the appropriate chemical detection devices to detect and monitor the chemicals on site. 
.2 The Contractor shall be responsible for supplying require personal protective equipment as required based on site conditions and applicable legislation.
Products – Not used
Execution – Not used
End of section
