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[bookmark: _Toc337361332][bookmark: _Toc379340445][bookmark: _Toc379340767][bookmark: _Toc379340860][bookmark: _Toc179777034]General
[bookmark: _Toc326725350][bookmark: _Toc326743636][bookmark: _Toc326743722][bookmark: _Toc330007300][bookmark: _Toc330275088][bookmark: _Toc330275401][bookmark: _Toc669216]Summary
This section outlines in general the work to be done under the Contract at the XXX XXX XXX located at XXX Main Street, Anytown, ON.
Recognize that the Work is to be performed in a water treatment/wastewater treatment/pumping station facility that must be kept in continuous uninterrupted operation. Plan and schedule the Work consistent with specified operational constraints and with the objective of uninterrupted operation of the Project Description.
Construct and test (foundations, structures, roads, ducts, pipelines, buildings, tanks, and other facilities) shown on the Drawings and specified herein.
Supervise, organize, co-ordinate and direct construction operations of Subcontractors and Suppliers.
Supply, install, and put in continuous successful operation equipment and appurtenances specified herein. Include operating assistance to Owner as described herein.
In addition to constructing the works shown on the Drawings, design, construct, and maintain, unless otherwise specified or shown on the Drawings, temporary works and facilities required for the construction of the works. Remove temporary works and facilities when construction is completed. Temporary works and facilities include, but are not limited to the following:
All security fencing whether permanent or temporary
Sheeting and shoring systems for excavations whether part or all is left in place or not
Construction roads, bridges, ramps, accesses, and similar items
Excavation dewatering systems
Formwork for concrete
Falsework and bracing for formwork or for other parts of the works while under construction
Bracing and shoring for partially completed masonry, steelwork, precast concrete, or other assembly
Scaffolding
Process bypass installation
Channel bulkheads
Electrical, instrumentation, and water services
Snow removals
Grass cutting
Temporary vehicular access and parking development, maintenance, and restoration
Erosion control measures
Work covered by Contract Documents
The completed Work will provide the Owner with a functioning WP/WPCP/PS plant.
Modify the following list to suit the scope of work identified in the summary of work.
The Contract includes but is not limited to the following work:
1. [bookmark: _Toc448543074][bookmark: _Toc448624581]Civil
Site preparation
Environmental Protection during construction period
Excavating, dewatering excavations, backfilling, and disposal of surplus materials
Piling systems
Grading, drainage, sodding and landscaping
Site drainage during construction
Maintaining existing roads used during construction and leaving these roads in as good a condition as they were prior to site work
Fencing, lighting, and site security
Structural
Watertightness testing
Architectural
Mechanical
Associated mechanical equipment
Mechanical systems
Heating, ventilation, and air conditioning
Process mechanical pumps
Piping
Valves
Electrical
Instrumentation and control systems
Furnishing of materials, equipment, tools, implements, and labour.
Submersible mixers
Commissioning
Warranty period
In general, the Project includes the following facilities:
1. Operations Facility (Administration and Laboratory), including potable water supply
Headworks (Influent Pumping, Screening and lighting)
Bioreactors
Secondary Clarifiers
Alum Chemical
Tertiary Filters
UV Disinfection
Each section of the Specifications is not necessarily complete in itself. Read each section in conjunction with all other Contract Documents. Also ensure that Subcontractors read the relevant documents and comply with the requirements.
[bookmark: _Toc326725351][bookmark: _Toc326743637][bookmark: _Toc326743723][bookmark: _Toc330007301][bookmark: _Toc330275089][bookmark: _Toc330275402][bookmark: _Toc669217]Work not covered by Contract Documents
The Owner will notify the Contractor of any work to be performed by others.
[bookmark: _Toc326725352][bookmark: _Toc326743638][bookmark: _Toc326743724][bookmark: _Toc330007302][bookmark: _Toc330275090][bookmark: _Toc330275403][bookmark: _Toc669218]Provisions for future work
[bookmark: EditPos]Provisions for future construction are included in Contract D20XX-XX as shown on Drawings. The future work will be tendered under a separate contract. The provisions for such future construction include the following:
1. Example: Channel connections for third bioreactor.
Example: Channel connections for additional tertiary filter cells and modules.
Equipment, material and services provided by the owner
The Contract Documents allow for an area on-site for the Contractor's use. The boundary limits must be strictly adhered to in order to minimize the impact to the natural conditions. If additional space is required, obtain agreement in writing from the Owner.
The cost of electricity, telephone, gas, or other utilities, whether temporary or permanent, used for heating, lighting, power tools, testing, or other construction related purposes, fencing, security, and conveniences, will be the responsibility of the Contractor. Provide storage facilities, unloading of equipment or materials, maintenance while in storage, installation, labour and maintenance after installation.
When required written notice is given, the Owner will take equipment out of service and isolate pipelines.
Draining and flushing of pipelines before removal or making connections is the Contractor's responsibility.
Contract Drawings
The Contract Drawings are prepared in SI metric units.
The Drawings have been grouped according to discipline: General, Civil, Structural, Architectural, Process, Mechanical (HVAC), Plumbing, Electrical, and Instrumentation and Control. Read the Drawings as a whole, since details applicable to one discipline may appear on the Drawings of another discipline.
The Drawings give general location of piping routes, ductwork routes, cable tray and raceway routes, and equipment. Except where specific dimensions are indicated, locate piping, ductwork, cable tray and raceway, and equipment to limit interference with existing equipment not to be removed, pedestrian access, crane routes, and required headroom.
Additional drawings showing details in accordance with which the Work is to be constructed may be supplied from time to time by the Owner or the Consultant. Such drawings are for the information of and assistance to the Contractor and will not become a basis for extra payment. The Owner or the Consultant may supply drawings covering additional work. These will be identified as additional work.
[bookmark: _Toc116804466]Contract Specifications
The Contract Specifications are divided into divisions. Read the Specifications as a whole as details applicable to one division may appear in another division or divisions.
Co-ordinate and be responsible for the work done by Subcontractors.
Work compliance
Provide Work conforming to the lines, levels and grades specified or shown on the Drawings.
Construct the Work in a thoroughly substantial and workmanlike manner, in accordance with the Drawings and Specifications, subject to such modifications and additions as may be deemed necessary during its execution. In no case will payment be made for Work in excess of the requirements of the Drawings and Specifications, unless approved in writing by Consultant.
Engineering design
Where Specifications require work to be designed by an engineer, engage a Professional Engineer licensed in the Province of Ontario to design such work.
[bookmark: _Toc116804469]Examination of existing conditions
The Contract Documents indicate the extent of work. However, it is the Contractor's responsibility to examine on site during the time of tendering to develop a full appreciation of the scope of work.
The routings are to be generally kept within existing tunnels and structures as far as practicable. The pipes and conduits are to be buried only in the absence of tunnel or building access to points shown on the Drawings.
Provincial standards
Ontario Provincial Standard Specifications (OPSS) and Ontario Provincial Standard Drawings (OPSD) current at the date of tendering shall apply to this Contract. OPSS and OPSD referenced or inferred within the Drawings and Specifications form part of the Contract Documents. The referenced OPSS and OPSD are not bound in the Contract Documents; however, the Contractor shall be required to comply with these specifications.
Regional standards
The Regional Municipality of Durham Construction Specifications for Regional Services (RMDCS) are not bound in the Contract Documents; however, the Contractor shall be required to comply with these specifications.
Work sequence
Contractor shall be allowed to determine their own method of construction within the terms of his Contract, as long as the constraints defined in Section 01 31 13 – Project Co-ordination are observed and the overall project completion time is achieved.
Conform to Section 01 32 13 – Scheduling of Work.
Conform to Section 01 32 16 – Construction Progress Schedule 
Contractor use of the premises
Contractor shall limit their use of the premises for the Work and for storage. Contractor shall allow for the Work performed by other contractors. Conform with Section 01 31 13 – Project Co-ordination.
Contractor shall perform Work within the limits identified. Contractor shall not work, store materials, or otherwise impact the adjacent lands unless specifically called for by the Contract Documents.
Warranty inspection
The Consultant will arrange and conduct with the Owner and the Contractor a warranty inspection at the site prior to the expiration of the warranty period. Any deficiencies or work identified during this inspection shall be remedied by the Contractor immediately at no cost to the Owner.
Inclement weather
Provide adequate protection for the Work and take precautions at times of inclement weather.
Products 
[bookmark: _Toc196993036]Non-U.S. Products
As a result of the ongoing U.S. tariff uncertainties, the Region is working to support the medium and long-term growth of Canadian suppliers as well as develop longer term alternatives to U.S. suppliers to ensure competition and a diverse supply chain. To that end, the Region is requesting suppliers take commercially reasonable efforts to avoid supplying products that come from the U.S.
The Supplier/Contractor shall take commercially reasonable steps to mitigate the costs and damages it may incur as a result of such tariffs by consulting with the Region to determine whether:
1. the goods can be sourced from countries to which the additional tariffs do not apply; and/or
the goods can be shipped and imported into Canada prior to effective date of the additional tariffs.
Execution – Not used
End of section
